IPC

Project TFS path: $/Firmware-SVI II AP FF/FIRMWARE

Project changeset version: 47651

Starting point: timeout monitoring

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Containing file | | FIRMWARE/interface/hart/hart\_ipc.c | Review Date | Reviewer |
| Function or data | | IPC\_RefreshTimeStamp | 15-05-13 | AK |
|  | | | | |
| TFS wit |  | Why is the critical section needed? | | |
| Impact | | Style, efficiency | | |
| Additional | | See also LOCAL UI IMPROVEMENTS | | |
| Resolution | |  | | |
|  | | | | |
| TFS wit |  | Why 3 calls? Isn’t only command 177 critical? What if only 177 doesn’t run? | | |
| Impact | | Weak monitoring of a critical failure | | |
| Additional | | See also LOCAL UI IMPROVEMENTS | | |
| Resolution | |  | | |